R2 Config

R2#sh run
Building configuration...

Current configuration : 2539 bytes
!
version 12.4
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname R2
!
boot-start-marker
warm-reboot
boot-end-marker
!
logging message-counter syslog
enable secret 5 $1$pMj4$EDxl19aKQpkQUxh9nxoXS1
!
no aaa new-model
memory-size iomem 15
!
dot11 syslog
ip source-route
ip cef
!
!
!
!
no ip domain lookup
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
voice-card 0
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
vtp domain null
vtp mode transparent
vtp version 2
archive
 log config
  hidekeys
! 
!
!
!
!
vlan 2,5 
!
vlan 7
 name DOT1XFAIL
!
vlan 8-13,16-17,20-23 
!
vlan 24
 name R2-R4
!
vlan 25-27,42,48-49,59,67,72,89 
!
vlan 100
 name OPS-100
!
vlan 101
 name OPS-101
!
vlan 102
 name OPS-102
!
vlan 110-112,200 
!
vlan 201
 name R2-BB1
!
vlan 210,222,230,241,250,252,300,302,440,444,555,900,902 
!
vlan 1004
 bridge 0
 stp type ieee
!
!
!
!
!
interface Loopback0
 ip address 200.0.0.2 255.255.255.255
!
interface GigabitEthernet0/0
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type sfp
 negotiation auto
!
interface GigabitEthernet0/1
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface Serial0/1/0
 description Frame Relay Links
 ip address 150.100.100.2 255.255.255.0
 encapsulation frame-relay
 frame-relay map ip 150.100.100.5 205 broadcast
 frame-relay map ip 150.100.100.6 206 broadcast
 frame-relay map ip 150.100.100.2 205
 no frame-relay inverse-arp
!
interface Serial0/1/0.1 point-to-point
 ip address 150.100.24.2 255.255.255.0
!
interface Serial0/2/0
 description Serial Link to R5
 no ip address
 shutdown
 clock rate 2000000
!
interface FastEthernet1/0
 shutdown
!
interface FastEthernet1/1
 shutdown
!
interface FastEthernet1/2
 shutdown
!
interface FastEthernet1/3
 shutdown
!
interface FastEthernet1/4
 shutdown
!
interface FastEthernet1/5
 shutdown
!
interface FastEthernet1/6
 shutdown
!
interface FastEthernet1/7
 shutdown
!
interface FastEthernet1/8
 shutdown
!
interface FastEthernet1/9
 shutdown
!
interface FastEthernet1/10
 shutdown
!
interface FastEthernet1/11
 shutdown
!
interface FastEthernet1/12
 shutdown
!
interface FastEthernet1/13
 shutdown
!
interface FastEthernet1/14
 shutdown
!
interface FastEthernet1/15
 shutdown
!
interface Vlan1
 no ip address
!
ip forward-protocol nd
ip http server
no ip http secure-server
!
!
!
!
!
!
!
!
!
control-plane
!
!
!
!
!
!
!
!
!
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login
!
scheduler allocate 20000 1000
end