Print file information:
RUN_IN_PLACE=no
EMC2_DIR=
EMC2_BIN_DIR=/usr/bin
EMC2_TCL_DIR=/usr/share/emc/tcl
EMC2_SCRIPT_DIR=
EMC2_RTLIB_DIR=/usr/realtime-2.6.32-122-rtai/modules/emc2
EMC2_CONFIG_DIR=
EMC2_LANG_DIR=/usr/share/emc/tcl/msgs
INIVAR=inivar
HALCMD=halcmd
EMC2_EMCSH=/usr/bin/wish8.5
EMC2 - 2.4.3
Machine configuration directory is '/home/farax-2/emc2/configs/my-mill'
Machine configuration file is 'my-mill.ini'
INIFILE=/home/farax-2/emc2/configs/my-mill/my-mill.ini
PARAMETER_FILE=stepper.var
EMCMOT=motmod
EMCIO=io
TASK=milltask
HALUI=halui
DISPLAY=axis
NML_FILE=
Starting EMC2...
Starting EMC2 server program: emcsvr
Loading Real Time OS, RTAPI, and HAL_LIB modules
Starting EMC2 IO program: io
Starting HAL User Interface program: halui
INFO CLASSICLADDER-   No ladder GUI requested-Realtime runs till HAL closes.
Shutting down and cleaning up EMC2...
Killing task emcsvr, PID=1785
Removing HAL_LIB, RTAPI, and Real Time OS modules
Removing NML shared memory segments
Cleanup done

Debug file information:
insmod: error inserting '/usr/realtime-2.6.32-122-rtai/modules/emc2/hal_parport.ko': -1 Resource temporarily unavailable
standard_pinout.hal:6: exit value: 1
standard_pinout.hal:6: insmod failed, returned -1
See the output of 'dmesg' for more information.
1785
  PID TTY      STAT   TIME COMMAND
Stopping realtime threads
Unloading hal components

Kernel message information:
[  609.097327] I-pipe: Domain RTAI registered.
[  609.097332] RTAI[hal]: <3.8.1> mounted over IPIPE-NOTHREADS 2.6-03.
[  609.097334] RTAI[hal]: compiled with gcc version 4.4.3 (Ubuntu 4.4.3-4ubuntu5) .
[  609.097356] RTAI[hal]: mounted (IPIPE-NOTHREADS, IMMEDIATE (INTERNAL IRQs DISPATCHED), ISOL_CPUS_MASK: 0).
[  609.097358] PIPELINE layers:
[  609.097360] faef5e20 9ac15d93 RTAI 200
[  609.097362] c085cb20 0 Linux 100
[  609.111913] RTAI[malloc]: global heap size = 2097152 bytes, <BSD>.
[  609.112291] RTAI[sched]: IMMEDIATE, MP, USER/KERNEL SPACE: <with RTAI OWN KTASKs>, kstacks pool size = 524288 bytes.
[  609.112296] RTAI[sched]: hard timer type/freq = APIC/12499668(Hz); default timing: periodic; linear timed lists.
[  609.112298] RTAI[sched]: Linux timer freq = 250 (Hz), TimeBase freq = 2700092000 hz.
[  609.112300] RTAI[sched]: timer setup = 999 ns, resched latency = 2943 ns.
[  609.112364] RTAI[usi]: enabled.
[  609.144144] RTAI[math]: loaded.
[  609.204677] creating ladder-state
[  609.218150] config string '0x378'
[  609.218163] PARPORT: ERROR: port parport0 claim failed
[  609.482368] RTAI[math]: unloaded.
[  609.507190] SCHED releases registered named ALIEN RTGLBH
[  609.536282] RTAI[malloc]: unloaded.
[  609.636017] RTAI[sched]: unloaded (forced hard/soft/hard transitions: traps 0, syscalls 0).
[  609.638376] I-pipe: Domain RTAI unregistered.
[  609.638404] RTAI[hal]: unmounted.