Hi All,

We have a SUN System that communicates with an OS/390 system using MQSeries.

The OS/390 and SUN systems have MQSeries5.2.

The Sun system has to send MQ messages with Logical Grouping (using the msgflags) to
the OS/390 system. We heard that the OS/390 system needs to use AMI calls to
retrieve messages using Logical Grouping. Is this true? Also should the application
that puts the message from the SUN System use AMI calls to put the message to the
OS/390 system? 

Since we are more bothered about our application on the SUN system, it would be 
helpful if someone could tell us if the "putting" application on SUN needs to use AMI
calls ( as the retrieving application on OS/390 is to use AMI) ?

Regards,
Lalithe.

GCX Application Support
Ph:91-44-8111393 (Extn 4015)
Mobile: 91-9840287422