A quem puder me ajudar.
Tenho esta configuração no meu roteador, e gostaria de saber o que significa essa configuração que destaquei entre parenteses, como posso ler p net que está abaixo do router isis, sei que uma parte diz respeito ao mac address, outra ao domínio, mas não sei identificar exatamente. O que siginifica as outras linhas?

Dúvidas.
(
router isis 23.6-CSER01
 net 39.032f.8000.0000.0000.0501.5065.0003.a00e.7400.00
!
router isis 23.6-CSER01-BWM
 net 39.840f.8011.3824.0000.0501.2280.0003.a00e.7400.00
 is-type level-1                                          )

( tarp run
 tarp tid riodj-23CSER01  )

(  ip kerberos source-interface any  )

Desde já agradeço a ajuda de todos.

Configuração do roteador.
!
version 12.1
no service single-slot-reload-enable
service timestamps debug uptime
service timestamps log uptime
no service password-encryption
!
hostname riodj-23CSER01
!
logging rate-limit console 10 except errors
enable secret 5 $1$7nx9$4Wku9aSVf3OW1dpmkdl2v/
enable password cisco
!
ip subnet-zero
!
!
no ip finger
!
clns routing
call rsvp-sync
cns event-service server
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 192.168.23.5 255.255.255.255
!
interface FastEthernet0/0
 no ip address
 no ip mroute-cache
 duplex half
!
interface FastEthernet0/0.12
 description IP port 9-16 on switch
 encapsulation isl 12
 ip address 172.23.6.130 255.255.255.192
 no ip redirects
 ip ospf cost 100
 standby 12 timers 5 15
 standby 12 priority 120 preempt
 standby 12 ip 172.23.6.129
 clns enable
!
interface FastEthernet0/0.14
 description OSI port 1 on switch to BWM
 encapsulation isl 14
 ip address 172.23.6.194 255.255.255.192
 no ip redirects
 standby 14 timers 5 15
 standby 14 priority 120 preempt
 standby 14 ip 172.23.6.193
 clns router isis 23.6-CSER01-BWM
 tarp enable
!
interface FastEthernet0/0.30
 description OSI-level 2 routing
 encapsulation isl 30
 no ip redirects
 clns router isis 23.6-CSER01
 isis circuit-type level-2-only
!
interface Ethernet1/0
 description connected to Ip lan
 ip address 172.23.6.2 255.255.255.192
 ip ospf cost 64
 duplex half
 standby 1 timers 5 15
 standby 1 priority 110 preempt
 standby 1 ip 172.23.6.1
!
interface Ethernet1/1
 description connected to Osi Lan
 ip address 172.23.6.66 255.255.255.192
 ip ospf cost 65
 duplex half
 standby 1 timers 5 15
 standby 1 priority 110 preempt
 standby 1 ip 172.23.6.65
 clns router isis 23.6-CSER01
 isis circuit-type level-1
 isis priority 127 level-1
!
interface Ethernet1/2
 no ip address
 shutdown
 duplex half
!
interface Ethernet1/3
 no ip address
 shutdown
 duplex half
!
interface ATM3/0
 description connected to Rio TH router
 no ip address
 atm clock INTERNAL
 no atm ilmi-keepalive
!
interface ATM3/0.3 point-to-point
 description connected to Rio TH router
 ip address 172.23.254.9 255.255.255.252
 pvc ip 3/1 
  encapsulation aal5snap
 !
 clns router isis 23.6-CSER01
 isis circuit-type level-2-only
!
interface ATM4/0
 description connected to Fortaleza router
 no ip address
 atm clock INTERNAL
 no atm ilmi-keepalive
!
interface ATM4/0.2 point-to-point
 description connected to Fortaleza router
 ip address 172.23.254.6 255.255.255.252
 pvc ip 2/1 
  encapsulation aal5snap
 !
 clns router isis 23.6-CSER01
 isis circuit-type level-2-only
!
router ospf 100
 log-adjacency-changes
 passive-interface Loopback0
 network 172.23.6.0 0.0.0.255 area 0
 network 172.23.254.0 0.0.0.255 area 0
 network 192.168.23.5 0.0.0.0 area 0
!
router isis 23.6-CSER01
 net 39.032f.8000.0000.0000.0501.5065.0003.a00e.7400.00
!
router isis 23.6-CSER01-BWM
 net 39.840f.8011.3824.0000.0501.2280.0003.a00e.7400.00
 is-type level-1
!
ip kerberos source-interface any
ip classless
ip http server
!
!
tarp run
tarp tid riodj-23CSER01
!
!
gatekeeper
 shutdown
!
!
line con 0
 exec-timeout 0 0
 password cisco
 login
 transport input none
line aux 0
line vty 0 4
 exec-timeout 0 0
 line vty 5 15
 login
!
end

     Roberto da Silva Liarth
         Service Engineer
   Alcatel Submarine Networks
 Roberto.Liarth@alcatel.com.br
  +55 (21)  442-2063   (Office)
  +55 (21)  442-2065   (Fax)